Silverado Alarm Wiring

WIRE          COLOR          POLARITY          LOCATION      
     Battery          RED/WHITE          (+)          IGNITION SWITCH HARNESS      
               LOW CURRENT, FOR HIGH CURRENT USE RED/BLACK AT VEHICLE FUSE BOX      


     Ignition 1          PINK          (+)          IGNITION SWITCH HARNESS      
     Accessory 1          BROWN          (+)          IGNITION SWITCH HARNESS      
               MAY BE YELLOW ON SOME MODELS      
     Accessory 2          PINK/BLACK          (+)          IGNTION SWITCH HARNESS      
               FOR REMOTE START INTEGRATION      
     Starter 1          YELLOW/BLACK          (+)          AT MODULE UNDER HOOD BEHIND DRIVER 

HEADLIGHT      
               NOT FOR REMOTE START, FOR REMOTE START INFORMATION      
     Starter 2          PINK/BLACK          (+)          IGNITION SWITCH HARNESS      
              

 FOR REMOTE START INTEGRATION      
     Anti-Theft Type          GM PASSKEY III® ANTI-THEFT SYSTEM      
     Anti-Theft Descript          THE KEY SENDS AN RF SIGNAL TO THE BCM MODULE THROUGH AN

ANTENNA LOCATED AROUND THE IGNITION CYLINDER      
     Key Sense          PINK          (+)          IGNITION SWITCH HARNESS      
     Tachometer          WHITE          (-)          AT IGNITION COIL      
     Speed Sense          YELLOW/BLACK          (AC)          AT ECM MODULE UNDER HOOD ON DRIVER 

FENDER      
               BLACK PLUG PIN #57      
     Parking Lights          LIGHT BLUE          (-)          AT VEHICLE LIGHT SWITCH      
     Brake Lights          LIGHT BLUE/WHITE          (+)          AT SWITCH ABOVE BRAKE PEDAL      
               IGNITION MUST BE ON FOR THIS WIRE TO TEST      
     Reverse Lights          DARK BLUE          (+)          AT BCM MODULE UNDER DRIVER DASH      
     Horn          TAN          (-)          IN HARNESS AT STEERING COLUMN      


ALSO AT BCM MODULE UNDER DRIVER DASH 
     All Door Trigger                
               MUST USE ALL TRIGGERS AND DIODE ISOLATE EACH WIRE      
     Domelight Super          GRAY          (+)          AT BCM MODULE UNDER DRIVER DASH      
     LF Latch          GRAY/BLACK          (-)          AT MODULE IN DRIVER DOOR      
     RF Latch          TAN/WHITE          (-)          AT MODULE IN PASSENGER DOOR      
               MAY BE BLACK/WHITE ON SOME MODELS      
     Hood Trigger          PINK/BLACK          (-)          AT BCM MODULE UNDER DRIVER DASH      
               BLACK PLUG PIN #17, NOT ON ALL MODELS      
     Alarm Disarm          LIGHT GREEN          (-)          AT MODULE IN DRIVERS DOOR      
     Parking Lights          LIGHT BLUE          (-)          AT VEHICLE LIGHT SWITCH
